<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="160" y2="0" width="0" layer="20"/>
<wire x1="160" y1="0" x2="160" y2="134.29" width="0" layer="20"/>
<wire x1="160" y1="134.29" x2="0" y2="134.29" width="0" layer="20"/>
<wire x1="0" y1="134.29" x2="0" y2="0" width="0" layer="20"/>
<text>Group 4 
"The Re-Suspension Riders"
PHYS371 - SP2023
Benson, Nussel, 
Raymundi Pinheiro,
Rodrigues De Almeida Prado
</text>
<text>Plantower</text>
<text>LCD</text>
<text>RTC DS3231</text>
<text>MicroSD
Breakout</text>
<text>Arduino Mega</text>
<text>LCD 
Trimpot</text>
<text>BME 680</text>
<text>Project in Collaboration with N.Dayega (UIUC &amp; ANL)</text>
<text>v1.0 - 22 Feb 2023</text>
<text>JLCJLCJLCJLC</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C5B5">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 7.5 x 5 mm, grid 5.08 mm</description>
</package>
</packages>
</library>
<library name="senba-pir-sensor">
<packages>
<package name="3PIN">
</package>
</packages>
</library>
<library name="GDG_library">
<packages>
<package name="GDG_ARDUINO_MEGA2560_PKG">
<description>Arduino MEGA 2560, component side DOWN</description>
</package>
<package name="GDG_PMS5003_PM2.5_PKG">
<description>PMS5003 airborne particulates sensor</description>
</package>
<package name="GDG_MICROSD_PKG">
<description>Adafruit microSD reader breakout board</description>
</package>
<package name="GDG_DS3231_PKG">
<description>DS3231 real time clock with battery backup</description>
</package>
<package name="GDG_LCD_16X2_PKG">
<description>2x16 liquid crystal display, four mounting holes. Crystalfontz CFAH1602B-NGG-JTV</description>
</package>
<package name="GDG_BME680_PKG">
<description>BME680 temperature, pressure, relative humidity, and volatile organic compounds sensor</description>
</package>
<package name="GDG_5XAA_BATTERY_PKG">
<description>Adafruit 5 x AA battery pack</description>
</package>
<package name="GDG_TRIMPOT_PKG">
<description>trimpot</description>
</package>
<package name="GDG_MOUNTING_HOLE_4MM_PKG">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C_BME" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C_LCD" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C_RTC" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="C_SD" library="capacitor-wima" package="C5B5" value="0.1uF">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="1"/>
<attribute name="VALUE"/>
</element>
<element name="PIR1" library="senba-pir-sensor" package="3PIN" value="D203B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="GDG_library" package="GDG_ARDUINO_MEGA2560_PKG" value="GDG_ARDUINO_MEGA2560_DEV"/>
<element name="U$2" library="GDG_library" package="GDG_PMS5003_PM2.5_PKG" value="GDG_PMS5003_PM2.5_DEV"/>
<element name="U$3" library="GDG_library" package="GDG_MICROSD_PKG" value="GDG_MICROSD_DEV"/>
<element name="U$4" library="GDG_library" package="GDG_DS3231_PKG" value="GDG_DS3231_DEV"/>
<element name="U$5" library="GDG_library" package="GDG_LCD_16X2_PKG" value="GDG_LCD_16X2_DEV"/>
<element name="U$6" library="GDG_library" package="GDG_BME680_PKG" value="GDG_BME680_DEV"/>
<element name="U$7" library="GDG_library" package="GDG_5XAA_BATTERY_PKG" value="GDG_5XAA_BATTERY_DEV"/>
<element name="U$8" library="GDG_library" package="GDG_TRIMPOT_PKG" value="GDG_TRIMPOT_DEV">
<attribute name="VALUE"/>
</element>
<element name="U$9" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$10" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$11" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
<element name="U$12" library="GDG_library" package="GDG_MOUNTING_HOLE_4MM_PKG" value=""/>
</elements>
<signals>
<signal name="PMS_D19RX1">
<contactref element="U$2" pad="TXD"/>
<contactref element="U$1" pad="D19RX1"/>
</signal>
<signal name="PMS_D18TX1">
<contactref element="U$2" pad="RXD"/>
<contactref element="U$1" pad="D18TX1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$5" pad="GND"/>
<contactref element="C_LCD" pad="2"/>
<contactref element="U$5" pad="R/W"/>
<contactref element="U$3" pad="3"/>
<contactref element="C_SD" pad="2"/>
<contactref element="U$6" pad="3"/>
<contactref element="C_BME" pad="2"/>
<contactref element="U$4" pad="2"/>
<contactref element="C_RTC" pad="2"/>
<contactref element="PIR1" pad="3"/>
</signal>
<signal name="5V">
<contactref element="U$1" pad="5V1"/>
<contactref element="C_LCD" pad="1"/>
<contactref element="U$5" pad="5V"/>
<contactref element="U$8" pad="BOTTOM"/>
<contactref element="U$3" pad="1"/>
<contactref element="C_SD" pad="1"/>
<contactref element="U$6" pad="1"/>
<contactref element="C_BME" pad="1"/>
<contactref element="U$4" pad="1"/>
<contactref element="C_RTC" pad="1"/>
<contactref element="U$2" pad="VCC"/>
<contactref element="PIR1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$8" pad="TAP"/>
<contactref element="U$5" pad="VO"/>
</signal>
<signal name="N$5">
<contactref element="U$8" pad="TOP"/>
<contactref element="U$5" pad="PULL"/>
</signal>
<signal name="LCD_DB4">
<contactref element="U$5" pad="DB4"/>
<contactref element="U$1" pad="D36"/>
</signal>
<signal name="LCD_DB5">
<contactref element="U$5" pad="DB5"/>
<contactref element="U$1" pad="D34"/>
</signal>
<signal name="LCD_DB6">
<contactref element="U$5" pad="DB6"/>
<contactref element="U$1" pad="D32"/>
</signal>
<signal name="LCD_DB7">
<contactref element="U$5" pad="DB7"/>
<contactref element="U$1" pad="D30"/>
</signal>
<signal name="SD_D51_DI">
<contactref element="U$3" pad="6"/>
<contactref element="U$1" pad="D51"/>
</signal>
<signal name="SD_D52_CLK">
<contactref element="U$1" pad="D52"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="SD_D50_DO">
<contactref element="U$1" pad="D50"/>
<contactref element="U$3" pad="5"/>
</signal>
<signal name="SD_D53_CS">
<contactref element="U$3" pad="7"/>
<contactref element="U$1" pad="D53"/>
</signal>
<signal name="I2C_SCL">
<contactref element="U$6" pad="4"/>
<contactref element="U$1" pad="D21SCL"/>
<contactref element="U$4" pad="3"/>
</signal>
<signal name="I2C_SDA">
<contactref element="U$6" pad="6"/>
<contactref element="U$1" pad="D20SDA"/>
<contactref element="U$4" pad="4"/>
</signal>
<signal name="LCD_RS">
<contactref element="U$1" pad="D12"/>
<contactref element="U$5" pad="RS"/>
</signal>
<signal name="LCD_E">
<contactref element="U$1" pad="D11"/>
<contactref element="U$5" pad="E"/>
</signal>
<signal name="PIR_OUT">
<contactref element="U$1" pad="D13"/>
<contactref element="PIR1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
